**ANNEX B**

**PRICING FORM**

**Retaining Wall Reconstruction South Rd Smith’s**

**2025**

**41-113-120**

Note: all blanks are to be filled in by the Contractor and all sheets form part of the BID

**August 2025**

# pricing form

(Note: all blanks are to be filled in by the Contractor and all sheets form part of the tender)

**Retaining wall reconstruction south rd smith’s**

NOTE: All work detailed on the contract documents shall be covered completely by the Grand Total. Individual lump sum items and rates are all-inclusive. If a specific task is not identified separately in the above list, the Contractor shall assume that it is included as part of another related listed item or items, or shall include it separately, and shall include it in the Grand Total amount.

LUMP SUM BID

**TO: PERMANENT SECRETARY, Ministry of Public Works**

Having examined the bid documents for the above work, we the undersigned, offer to construct and complete the whole of the said works for the lump sum of:

 (figures) BD$\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(words) BD$\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

We agree to abide by this bid for **thirty (30) calendar days** from the date fixed for receipt of bids, and understand that you may accept or reject any bid you may receive. We undertake to commence the works within fourteen calendar days of award of the Contract, and to complete the works by .

**Signed:**

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Block letters: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**On Behalf Of:**

Company name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Date:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Price Schedule

(To Be Completed By The Contractor)

All prices (in Bermuda dollars) are to be all inclusive of all other associated works as shown on the Contract Documents, materials, related accessories, storage, transport, assembly, placement, overhead and profit. These rates may be used for determining additions and deletions from the contract sum and for interim payment valuation.

| **ITEM** | **DESCRIPTION** |  **LUMP SUM** |
| --- | --- | --- |
|  | **Mobilization** |
| 1.1 | Equipment rental |  |
| 1.2 | Establishment of temporary facilities |  |
| 1.3 | Establishment of working site boundaries including fencing, temporary pedestrian pathways etc.  |  |
| 1.4 | Other items (please list below) |  |
|  |  |  |
|  | **Traffic Control** |
| 2.1 | Install and operate necessary measures to maintain vehicle access |  |
| 2.2 | Manual traffic control for the duration |  |
| 2.3 | Other items (please list below) |  |
|  |  |  |
|  | **Demolition and Excavation**  |
| 3.1 | Excavate to required lines and levels as shown in drawings |  |
| 3.2 | Demolish existing stone walls |  |
| 3.3 | Other items (please list below) |  |
|  |  |  |
|  | **Construction of Retaining Wall** |
| 4.1 | Construct concrete footing |  |
| 4.2 | Construct block wall with required reinforcement and bond beam |  |
| 4.3 | Construct unreinforced wall above grade |  |
| 4.4 | Plaster/paint and slate finishes |  |
| 4.5 | Other items (please list below) |  |
|  |  |  |
| **5.** | **Backfill and Site Grading**  |  |
| 4.1 | Backfill and compact as per the drawings |  |
| 4.2 | Supply asphalt material (sourced from Govt. plant) |  |
| 4.3 | Install asphalt as per the drawings |  |
|  |  |  |
| **6.** | **Demobilization and Site Clean-up** |
| 6.1 | Remove and dispose of waste |  |
| 6.2 | Demobilize equipment and facilities |  |
| 6.3 | Site clean-up |  |
| 6.4 | Other items (please list below) |  |
|  |  |  |
| **7.** | **Any items not listed above.** |
| 7.1 |  |  |
| 7.2 |  |  |
| 7.3 |  |  |
| 7.4 |  |  |
|  | **SUB-TOTAL**  |  |
|  | PROVISIONAL: Vegetation Removal |  |
|  | **TOTAL** |  |

SCHEDULE OF UNIT RATES

(to be completed by the contractor)

All prices (in Bermuda dollars) in the schedule are to be **inclusive of materials and related accessories, storage, transport, plant and equipment assembly, placement, access, overhead and profit.** These rates may be used for determining additions to, and deletions from, the contract sum.

 **ITEM UNIT RATE**

1. **Labour**
	1. Unskilled Labour Hr $\_\_\_\_\_\_\_\_\_\_\_
	2. Skilled Labour Hr $\_\_\_\_\_\_\_\_\_\_\_
	3. Supervisor Hr $\_\_\_\_\_\_\_\_\_\_\_
	4. Project Manager Hr $\_\_\_\_\_\_\_\_\_\_\_
2. **Equipment**
	1. Wheeled Loader Hr $\_\_\_\_\_\_\_\_\_\_
	2. Excavator Hr $\_\_\_\_\_\_\_\_\_\_
	3. Telehandler Hr $\_\_\_\_\_\_\_\_\_\_
	4. Generator Day $\_\_\_\_\_\_\_\_\_\_
	5. Other Equipment not listed above. Please list below:

 Hr / Day $\_\_\_\_\_\_\_\_\_\_

 Hr / Day $\_\_\_\_\_\_\_\_\_\_

 Hr / Day $\_\_\_\_\_\_\_\_\_\_

1. **Other Items not listed above**
	1. Excavation of soil yd3 $\_\_\_\_\_\_\_\_\_\_\_
	2. Vegetation management yd3 $\_\_\_\_\_\_\_\_\_\_\_
	3. Supply / install concrete yd3 $\_\_\_\_\_\_\_\_\_\_\_
	4. Supply / install masonry yd3 $\_\_\_\_\_\_\_\_\_\_\_
	5. Supply / install slate finish sqft $\_\_\_\_\_\_\_\_\_\_\_
	6. Supply / install plaster finish sqft $\_\_\_\_\_\_\_\_\_\_\_
	7. Supply and install 10mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_
	8. Supply and install 12mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_
	9. Supply and install 16mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_
	10. Supply and install 20mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_

All unit rates above shall be considered fully inclusive of delivery, preparation, placing and finishing.

For variations to the contract not covered in the preceding price break down rates or the above schedule of unit rates, the price may be determined on the basis of the base material and installation cost plus  **%** for overhead and  **%** for profit and applied separately to the base cost.